

1.End devices:


Add server:




2.network devices-switch –PTSwitch




Add PC0:




ADD PC1:




Add PC2:




Add Laptop0:




Add Laptop1:




Connection-Connect Copper Straight Wire




Switch OFF:




Add two Port:




Add Switch ON:




Connect Copper straight Wire to PC2 and Server:




IP Name for server:




DHCP-Service ON-Default Gateway-198.168.0.1




DNS-10.0.0.1





Save:



PC-Desktop-DHCP:







Add Packet:

